**WIRE & CABLE INSTALLATION**

**Conduit Systems –** Type THWN wires are to be used inside underground electrical conduit. A waterproof junction box must be installed inside the valve boxes and it must be connected to the conduit using a solvent weld or other approved waterproof connection method. The junction box must be fitted with a sealed lid.

