**Connectors for Decoder Cable Fuse Devices –** All splices made to connect electrical wires from the Decoder Cable Fuse Devices to the 2-Wire paths shall be made using the 3M Model DBR/Y-6. The 2-Wire cables shall have enough slack so as to extend a minimum of 36” above ground, for ease of making splices and for future maintenance. The Decoder Cable Fuse Devices shall be installed in a valve box. See installation illustration below.

**3M Model DBR/Y-6 (Paige Electric 270672.) No equal.**

