**POWER WIRES AND CABLES**

**Type UF-B Cable (*120 VAC systems only*) –** All branch circuit power cables shall be type UF-B. They are to be listed for direct burial, and rated at 600 volts. Wire sizes are defined in the irrigation plans and other specifications.

**Paige Electric Co., LP specification number P7295D, or approved equal.**

