**VALVE CONTROL WIRES**

**Single Conductors, Type UF/TWU –** Wires connecting the remote control valves to the irrigation controller shall be single conductors, type UF. The wires shall be listed for direct burial in irrigation systems and be rated at a minimum of 600 VAC. Wire sizes and colors are defined in the irrigation plans and other specifications.

**Paige Electric Co., LP specification number P7001D, or approved equal.**

