**VALVE CONTROL WIRES**

**Single Conductors, Type PE –** Wires connecting the remote control valves to the irrigation controller shall be single conductors, type PE. The wires shall be listed as “Golf Course Sprinkler Wire” for direct burial in irrigation systems and be rated at a minimum of 30 VAC. Wire sizes and colors are defined in the irrigation plans and other specifications.

**Paige Electric Co., LP specification number P7079D, or approved equal.**

