**CENTRAL-SATELLITE COMMUNICATION CABLES**

No Communication Cable underground splices are allowed unless it is necessary to make a repair. All repair splices shall be inside valve boxes and noted on the as-built.

**Cable for Rain Bird “Maxicom” Systems -** The communication cable shall be 19AWG with 3-pairs or 6-pairs, as shown on the plans. The cable construction shall be type PE-39 or PE-54 or PE-89.   
**Paige Electric Co., LP specification number P7315D, or approved equal.**

