**DECODER CABLES**

**Twisted Pair Cable for Hunter Decoder Systems –** The decoder cable shall consist of 2 wires, twisted together. Its construction incorporates solid copper conductors with PE insulation with a minimum wall thickness of 0.060”. The cable shall be listed for direct burial in irrigation systems and be rated at a minimum of 600 VAC. The cable shall be 14AWG/2c unless otherwise called-for in the irrigation plans and specifications

**Paige Electric Co., LP specification number P7313D. No equal.**

