**WIRE & CABLE SPLICES**

All electrical connectors for the irrigation system shall be listed under “UL486D-Direct Burial”, where applicable. This shall also apply to above ground splices that are in wet or damp locations. NO EXCEPTIONS.

Connectors for specific applications may have additional requirements, as detailed in the WIRE & CABLE SPLICES section to follow.

The contractor shall install these products per the instructions provided by the manufacturer of each product.

